Summary of Changes

Effective April 27, 2016, CenturyLink will post Revised Tech Specs and Summary of Changes.

CenturyLink will modify product based edits including, but not limited to, the following:

*Please NOTE: A complete list of EASE custom edits can be viewed by clicking on the web-link for ASR CenturyLink Custom Business Rules available from the EASE Homepage in the Guide (ASR) TAB.*

| **Action** | **ASR Form** | **Field**  | **Business Rule / WEBCALL / EDIT** | **Error Code** |
| --- | --- | --- | --- | --- |
| NEW | TRUNKING | CIC | THE TRUNK.CIC FIELD IS PROHIBITED WHEN THE ASR.WST FIELD IS POPULATED | EQ894 |
| NEW | TRUNKING | CIC | THE TRUNK.CIC FIELD IS PROHIBITED WHEN THE ASR.WST FIELD IS POPULATED | EQ895 |
| CHANGE | ACI | HBAN | THE LENGTH OF THIS FIELD IS INVALID | EQ003 |
| CHANGE | ASR | ACTL | THE LENGTH OF THIS FIELD IS INVALID | EQ003 |
| CHANGE | ASR | BAN | THE LENGTH OF THIS FIELD IS INVALID | EQ003 |
| CHANGE | EVC | EVCSP | THE LENGTH OF THIS FIELD IS INVALID | EQ003 |
| CHANGE | TRANS | HBAN | THE LENGTH OF THIS FIELD IS INVALID | EQ003 |
| CHANGE | TRUNK | FACTL | THE LENGTH OF THIS FIELD IS INVALID | EQ003 |
| CHANGE | TRUNK | HBAN | THE LENGTH OF THIS FIELD IS INVALID | EQ003 |
| CHANGE | ACI | CCEA | CCEA MUST CONTAIN VIRGULE | EQS10 |
| CHANGE | ACI | SCCEA | CCEA MUST CONTAIN VIRGULE | EQS10 |
| CHANGE | EUSA | CCEA | CCEA MUST CONTAIN VIRGULE | EQS10 |
| CHANGE | TRANSPORT | CCEA | CCEA MUST CONTAIN VIRGULE | EQS10 |
| CHANGE | TRANSPORT | SCCEA | CCEA MUST CONTAIN VIRGULE | EQS10 |
| CHANGE | TRUNK | CCEA | CCEA MUST CONTAIN VIRGULE | EQS10 |
| CHANGE | EUSA | SCCEA | SCCEA MUST CONTAIN VIRGULE | EQS11 |
| CHANGE | ACI | CCEA | CCEA 2ND SEGMENT MUST CONTAIN ONE OF THE FOLLOWING NL, COAX, OR LGSS | EQS8 |
| CHANGE | EUSA | CCEA | CCEA 2ND SEGMENT MUST CONTAIN ONE OF THE FOLLOWING NL, COAX, OR LGSS | EQS8 |
| CHANGE | TRANSPORT | CCEA | CCEA 2ND SEGMENT MUST CONTAIN ONE OF THE FOLLOWING NL, COAX, OR LGSS | EQS8 |
| CHANGE | TRUNK | CCEA | CCEA 2ND SEGMENT MUST CONTAIN ONE OF THE FOLLOWING NL, COAX, OR LGSS | EQS8 |
| CHANGE | ACI | SCCEA | SCCEA 2ND SEGMENT MUST CONTAIN ONE OF THE FOLLOWING NL, COAX OR LGGS | EQS9 |
| CHANGE | EUSA | SCCEA | SCCEA 2ND SEGMENT MUST CONTAIN ONE OF THE FOLLOWING NL, COAX OR LGGS | EQS9 |
| CHANGE | TRANSPORT | SCCEA | SCCEA 2ND SEGMENT MUST CONTAIN ONE OF THE FOLLOWING NL, COAX OR LGGS | EQS9 |
| CHANGE | ASR | SPEC | ASR SPEC VALUE MUST EQUAL EVPLD1, EVPLD2, EVPLD3, EVPLD4 WHEN SEI IS Y | EQ774 |
| CHANGE | EVC | SPEC | EVC SPEC VALUE MUST EQUAL EVPLD1, EVPLD2, EVPLD3, EVPLD4 WHEN EVCI=A | EQ775 |
| CHANGE | ASR | SPEC | WHEN SEI = Y THE ASR SPEC VALUE MUST EQUAL ONE OF EVPLC, EVPLN, BGPLU, ERPSC, MOENN, NONTLS, SVCPRV, SVCMUX, TLSMOE, TLSPLS, MCLAGAS | EQ637 |
| DELETE | ASR | NAG | CENTURYLINK ONLY SUPPORTS NAG FOR REQTYPE S ACT OF C | EQ445 |
| DELETE | ASR | NAG | CENTURYLINK ONLY SUPPORTS NAG FOR REQTYPE S ACT OF C | EQ446 |